**U-Joint and CV Joint Service**

**Meets ASE Task:** (A3-E-3.2) P-1, (A3-E-3.3) P-2, (A3-E-3.4) P-2, (A3-E-3.5) P-2 Inspect, service, and replace shafts, shaft center support bearings yokes, boots, and CV joints; check shaft balance and phasing.

**Name \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date \_\_\_\_\_\_\_\_\_\_\_ Time on Task \_\_\_\_\_\_\_\_\_\_**

**Make/Model/Year \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ VIN \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Evaluation: 4 3 2 1**

**\_\_\_\_\_ 1.** Check service information and determine the specified procedures, tools, and torque

 specification needed to service CV joints.

 Specified procedure: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Tools/equipment: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Torque specification: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**\_\_\_\_\_ 2.** Following the specified procedure, remove the drive axle shaft assembly.

 Instructor’s check \_\_\_\_\_\_\_\_\_\_\_\_

**\_\_\_\_\_ 3.** Following the specified installation procedure, check all that were replaced.

 \_\_\_ Drive axle shaft assembly \_\_\_ CV joint and boot

 \_\_\_ CV joint boot only \_\_\_ Other (specify) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**\_\_\_\_\_ 4.** Reinstall the drive axle shaft assembly.

 Instructor’s OK \_\_\_\_\_\_\_\_\_\_\_\_\_\_