[ ]  1. Retrieve the DTCs using a scan tool. Fault codes may be found in the PCM or the HVAC control module.

Evaluation (Enter number from 4, 3, 2, 1) :\_\_\_\_\_\_\_\_\_

Meets ASE Task: A7 – A-3 – P-1

Time on Task:\_\_\_\_\_\_\_\_\_\_\_\_\_

Make/Model/Year:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

VIN:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_

Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Retrieve and Record Diagnostic Trouble Codes**

 Specify which scan tool was used: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_

[ ]  2. If no DTCs are displayed, set a DTC by disconnecting a sensor such as the refrigerant pressure sensor and then starting the engine and running the climate control system.

[ ]  3. Did the scan tool display both a generic OBD II (Poxxx) code *and* a manufacturer’s specific DTC (P1xxx) code? **Yes \_\_\_\_\_ No \_\_\_\_\_**

 [ ]  4. Clear the stored DTCs using the scan tool.

