[ ]  1. Drill a hole in a piece of metal about ¼ inch thick and then thread it using a tap.

Meets ASE Task: (A0-B-6) Perform thread repair. Perform common fastener and thread repair, including removing broken bolts, restoring internal and external threads, and repairing internal threads with a thread insert.

**Thread Repair**

Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_

Time on Task:\_\_\_\_\_\_\_\_\_\_\_\_\_

Make/Model/Year:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

VIN:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Evaluation (Enter number from 4, 3, 2, 1) :\_\_\_\_\_\_\_\_\_

Page 11

 Install a bolt into the thread hole and either break it off or cut the bolt flush with the

 surface.

 Drill size \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Tap Size \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ **Instructor OK \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

[ ]  2. Remove the broken off bolt using an easy out or other tool.

 **Instructor OK \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

[ ]  3. Using an old engine block, drill out one threaded hole in the block and install a

 threaded insert, following the instructions that came with the thread insert kit.

 **Instructor OK \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**