**Meets ASE Task:** (A6-B-4) P-1 Inspect and clean battery; fill battery cells (if applicable); check battery cables, connectors, clamps, and hold-downs.

Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_

Time on Task:\_\_\_\_\_\_\_\_\_\_\_\_\_

Make/Model/Year:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

VIN:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Evaluation (Enter number from 4, 3, 2, 1) :\_\_\_\_\_\_\_\_\_

**Service and Replace the Battery**

Page 148

**[ ]  1.** Check service information for the specified procedures to follow to inspect, clean, fill,

 and replace a battery.

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**[ ]  2.** Check all that apply:

 **[ ]** Battery hold-down clamps/brackets are in place

 **[ ]** Filler cap(s) is removable

 **[ ]** Battery electrolyte cannot be checked

 **[ ]** Electrolyte level is low

 **[ ]** Corrosion was found on battery terminals/cable ends

 **[ ]** Other faults or conditions (describe)

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**[ ]  3.** Clean the battery.

**[ ]  4.** Clean the battery cables and cable ends.

**[ ]  5.** Remove and install the battery.