**Meets ASE Task:** (A6-B-6) P-1 Jump-start vehicle using jumper cables and a booster battery or an auxiliary power supply.

Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_

Time on Task:\_\_\_\_\_\_\_\_\_\_\_\_\_

Make/Model/Year:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

VIN:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Evaluation (Enter number from 4, 3, 2, 1) :\_\_\_\_\_\_\_\_\_

**Jump Starting**

Page 150

**[ ]  1.** Move the good vehicle to within reach of the jumper cables of the disabled vehicle (or

 use a portable jumper box).

**[ ]  2.** Check that the ignition is in the “off” position on both vehicles.

**[ ]  3.** Connect the jumper cables in the following order:

 a. Red cable ends to the positive (+) terminals of both batteries

 b. One black cable end to the negative (-) terminal of the good vehicle

 c. The other black cable end to a good, unpainted engine ground at least one

 foot from the battery

**[ ]  4.** Start the good vehicle.



**[ ]  5.** Allow the good vehicle to run for

 several minutes to charge the battery

 of the disabled vehicle.

**[ ]  6.** Start the disabled vehicle.

**[ ]  7.** After the engine is running smoothly,

 disconnect the black cable from the

 engine ground of the disabled vehicle

 and then disconnect the negative

 terminal of the battery of the good

 vehicle.

**[ ]  8.** Disconnect the red battery cable ends from the positive terminals of the batteries.