**Meets ASE Task: :** (A6-C-3) P-2 Inspect and test starter relays and solenoids; determine needed action.

Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_

Time on Task:\_\_\_\_\_\_\_\_\_\_\_\_\_

Make/Model/Year:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

VIN:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Evaluation (Enter number from 4, 3, 2, 1) :\_\_\_\_\_\_\_\_\_

**Starter Relays and Solenoids**

Page 157

**[ ]  1.** Clean and visually inspect the starter solenoid and/or relay for physical damage.

 **OK [ ]  NOT OK [ ]**

**[ ]  2.** Set a digital multimeter (DMM) to read ohms (low scale) and check the hold-in coil

 and the pull-in coil.

 **Pull-in coil. M**easure between terminals “S” and “M”:

 resistance = \_\_\_\_\_\_ (should be 0.2 to 0.4 ohm) **OK [ ]  NOT OK [ ]**

 **Hold-in coil.** Measure between terminals “S” and the solenoid housing:

resistance = \_\_\_\_\_\_\_ (should be 0.4 to 0.6 ohm) **OK [ ]  NOT OK [ ]**

**[ ]  3.** Test the pull-in winding by applying 12 volts to terminal “S” and ground to terminal

 “M.” Check that the plunger will be drawn into the solenoid.



**OK [ ]  NOT OK [ ]**

**[ ]  4.** Check the hold-in winding by connecting 12 volts

 to terminal “S” and the other wire to ground. The

 plunger should be drawn into the solenoid housing.

 **OK [ ]  NOT OK [ ]**

**[ ]  5.** Measure coil resistance of the relay (terminals 86 and

 85).

 Resistance = \_\_\_\_\_\_ ohms

 (should be 60 to 100 ohms)

**OK [ ]  NOT OK [ ]**

**[ ]  6.** What is the needed action?

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_