**Meets ASE Task:** (A6-G-4) P-1 Describe disabling and enabling procedures for supplemental restraint system (SRS); verify indicator lamp operation.

Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_

Time on Task:\_\_\_\_\_\_\_\_\_\_\_\_\_

Make/Model/Year:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

VIN:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Evaluation (Enter number from 4, 3, 2, 1) :\_\_\_\_\_\_\_\_\_

**Disarm and Enable Airbags**

Page 183

Airbags should be temporarily disabled whenever working

on or around the steering column or dash areas of a vehicle

equipped with airbags.

**[ ]  1.** Check service information for the specified method

 to use to disarm and enable the airbags.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**[ ]  2.** Disconnect the negative (-) battery cable.

**[ ]  3.** Locate and remove the airbag fuse.

Label of fuse = \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Amperage rating of the fuse = \_\_\_\_\_\_\_\_\_\_\_\_

**[ ]  4.** Remove the covering from underneath the steering column to gain access to the

 steering column airbag wiring connector.

**[ ]  5.** Disconnect the yellow airbag electrical connector.

**[ ]  6.** Locate and disconnect the yellow passenger side airbag electrical connector.

Describe the location \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

What components had to be removed to gain access to the passenger side airbag connector? \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**[ ]  7.** After servicing the steering column or dash, restore the airbags by reconnecting the

 connectors, installing the airbag circuit fuse, and reconnecting the battery.

**[ ]  8.** Start the engine and check for proper operation of the airbag warning light.

**OK [ ]  NOT OK [ ]**