**Meets ASE Task:** (A8-D-9) P-1 Inspect throttle body, air induction system, intake manifold and gaskets for vacuum leaks and/or unmetered air.

Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_

Time on Task:\_\_\_\_\_\_\_\_\_\_\_\_\_

Make/Model/Year:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

VIN:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Evaluation (Enter number from 4, 3, 2, 1) :\_\_\_\_\_\_\_\_\_

**Air Intake Inspection**

Page 249

The idle air control is used to control idle speed by increasing or decreasing the amount of air entering the engine like what occurs when the accelerator pedal is depressed.

**[ ]  1.** Inspect throttle body and related components for vacuum leaks.

**OK** **[ ]  NOT OK** **[ ]** Describe faults: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_



**[ ]  2.** Connect a scan tool.

**[ ]  3.** Look at the IAC commanded position

 = \_\_\_\_\_\_\_\_ (should be 15 to 25% or counts

 on a warm engine in park or neutral).

 **OK** **[ ]  NOT OK** **[ ]**

**Diagnosis:**

* **IAC counts higher than normal.** This could indicate one or more of the following:

1. Engine not fully warm

2. Some electrical load is on, such as daytime running lights or air

 conditioning

3. Dirty throttle plates

4. Abnormal load on the engine

* **IAC counts lower than normal.** This could indicate one or more of the following:

1. A vacuum leak

2. Misadjusted idle speed control

3. Stuck or binding throttle cable or linkage

**[ ]  4.** Based on the inspection of the system, what is the needed action? \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_