Evaluation (Enter number from 4, 3, 2, 1) :\_\_\_\_\_\_\_\_\_

**Meets ASE Task:** (A6-G-5) P-1 Verify windshield wiper and washer operation; replace wiper blades.

**Windshield Wiper Blade Service**

Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_

Time on Task:\_\_\_\_\_\_\_\_\_\_\_\_\_

Make/Model/Year:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

VIN:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Page 33

**1.** Turn the ignition switch on (engine off). Pull both wipers t their forward/non-contact

position.

**2.** Turn the wiper switch on and operate the wipers. As soon as the wiper arms are in an

accessible location on the windshield, turn off the ignition switch.

**3.** Carefully inspect the condition of the wiper blades.

**OK  NOT OK**

**4.** If they are OK (serviceable), use a clean shop cloth and windshield washer fluid to

wipe the blades to remove road grime.

**5.** If the wiper blades need replacing, measure the length.

Left (driver) side = \_\_\_\_\_\_\_\_\_ Right (passenger) side = \_\_\_\_\_\_\_\_\_\_

**6.** Describe how the replacement wiper blade inserts are removed and replaced.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**7.** After servicing the wipers, turn the ignition switch on and observe the wipers for

proper operation.

**OK  NOT OK**

**8.** Turn the wiper switch to off and allow the wiper to park.

**9.** Turn the ignition switch to the off position.