Evaluation (Enter number from 4, 3, 2, 1) :\_\_\_\_\_\_\_\_\_

**Meets ASE Task:** (A6-G-5) P-1 Verify windshield wiper and washer operation; replace wiper blades.

**Windshield Wiper Blade Service**

Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_

Time on Task:\_\_\_\_\_\_\_\_\_\_\_\_\_

Make/Model/Year:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

VIN:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Page 33

**[ ]  1.** Turn the ignition switch on (engine off). Pull both wipers t their forward/non-contact

 position.

**[ ]  2.** Turn the wiper switch on and operate the wipers. As soon as the wiper arms are in an

 accessible location on the windshield, turn off the ignition switch.

**[ ]  3.** Carefully inspect the condition of the wiper blades.

 **OK [ ]  NOT OK [ ]**

**[ ]  4.** If they are OK (serviceable), use a clean shop cloth and windshield washer fluid to

 wipe the blades to remove road grime.

**[ ]  5.** If the wiper blades need replacing, measure the length.

 Left (driver) side = \_\_\_\_\_\_\_\_\_ Right (passenger) side = \_\_\_\_\_\_\_\_\_\_

**[ ]  6.** Describe how the replacement wiper blade inserts are removed and replaced.

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**[ ]  7.** After servicing the wipers, turn the ignition switch on and observe the wipers for

 proper operation.

 **OK [ ]  NOT OK [ ]**

**[ ]  8.** Turn the wiper switch to off and allow the wiper to park.

**[ ]  9.** Turn the ignition switch to the off position.