Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_

Time on Task:\_\_\_\_\_\_\_\_\_\_\_\_\_

Make/Model/Year:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

VIN:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Evaluation (Enter number from 4, 3, 2, 1) :\_\_\_\_\_\_\_\_\_

**Meets ASE Task: :** (A4-F-6) P-1 Dismount, inspect, and remount tire on wheel (with/without TPMS); balance wheel and tire assembly.

**Tire Replacement**

Page 340

1. Check the instructions for the proper use of the tire changer. Describe the


recommended procedure.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

2. Check all steps that were performed.

Removed the valve core (TPMS equipped tire/wheel assembly; check

 service information for the exact procedure to follow.)

Demount the tire from the wheel. Instructor OK \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

  Clean bead seat.

Lubricate the tire bead.

Mount the tire and inflate to

specified inflation pressure.

3. Balance tire/wheel assembly.

Instructor OK \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_