Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_

Time on Task:\_\_\_\_\_\_\_\_\_\_\_\_\_

Make/Model/Year:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

VIN:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Evaluation (Enter number from 4, 3, 2, 1) :\_\_\_\_\_\_\_\_\_

**Meets ASE Task: :** (A3-D-2) P-1 Inspect, service, and/or replace shafts, yokes, boots, and universal/CV joints.

**U-Joint and CV Joint Service**

Page 395

**1.** Check service information and determine the specified procedures, tools, and torque

specification needed to service CV joints.

Specified procedure: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Tools/equipment: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Torque specification: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**2.** Following the specified procedure, remove the drive axle shaft assembly.

 Instructor’s check \_\_\_\_\_\_\_\_\_\_\_\_

**3.** Following the specified installation procedure, check all that were replaced.

Drive axle shaft assembly CV joint and boot

CV joint boot only Other (specify) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**4.** Reinstall the drive axle shaft assembly.

Instructor’s OK \_\_\_\_\_\_\_\_\_\_\_\_\_\_