Evaluation (Enter number from 4, 3, 2, 1) :\_\_\_\_\_\_\_\_\_

**Meets ASE Task:** (A1-D-2) P-1 Perform engine oil and filter change; use proper fluid type per manufacturer specification; reset maintenance reminder as required.

**Engine Oil Change**

Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_

Time on Task:\_\_\_\_\_\_\_\_\_\_\_\_\_

Make/Model/Year:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

VIN:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Page 58

**[ ]  1.** Check the owner's manual, service manual, or technical literature to determine the

 correct viscosity rating and quantity of oil needed.

1. Recommended viscosity: SAE \_\_\_\_\_\_\_ or SAE \_\_\_\_\_\_\_\_
2. Number of quarts (liters): with the filter \_\_\_\_\_\_ without the filter \_\_\_\_\_\_
3. American Petroleum Institute rating (if specified) \_\_\_\_\_\_\_\_\_\_\_

**[ ]  2.** Filter brand and number: Brand \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Number \_\_\_\_\_\_\_\_\_\_\_\_\_

**[ ]  3.** Hoist the vehicle safely. Position the oil drain unit under the drain plug and raise to a

 height about 1 foot under the drain plug.

**[ ]  4.** Select the proper size wrench and remove the drain plug and allow the oil to drain into

 the drain pan.

**[ ]  5.** After all the oil has been drained, install a new sealing washer (if needed) and install

 the drain plug.

**[ ]  6.** Move the oil drain unit under the filter and remove the old oil filter.

**[ ]  7.** Use a shop cloth and clean the oil filter gasket contact area on the engine block.

**[ ]  8.** Apply a thin coating of engine oil to the rubber gasket on the new oil filter.

**[ ]  9.** Install the new oil filter and hand tighten about 3/4 turn after the gasket contacts the

 engine block.

**[ ]  10.** Lower the vehicle. Install the recommended quantity of engine oil using a funnel to

 prevent spilling oil. Replace the oil filler cap.

**[ ]  11.** Start the engine and allow it to idle. The "oil" light should go out within 15 seconds.

**[ ]  12.** Look under the vehicle and check for leaks at the drain plug and the oil filter.

**[ ]  13.** Check the level of the oil again and add as needed. **Caution:** Do not overfill!