[ ]  1. Check service information for the specified procedures to follow to inspect, clean, fill, and replace a battery.

Evaluation (Enter number from 4, 3, 2, 1) :\_\_\_\_\_\_\_\_\_

Meets ASE Task: A6 – B-4 – P-1

Time on Task:\_\_\_\_\_\_\_\_\_\_\_\_\_

Make/Model/Year:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

VIN:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_

Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Service and Replace the Battery**

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

[ ]  2. Check all that apply:

 [ ] \_\_\_\_ Battery hold-down clamps/brackets are in place.

 [ ] \_\_\_\_ Filler cap(s) is removable.

 [ ] \_\_\_\_ Battery electrolyte cannot be checked

 [ ] \_\_\_\_ Electrolyte level is low.

 [ ] \_\_\_\_ Corrosion was found on battery terminals/cable ends.

 [ ] \_\_\_\_ Other faults or conditions (describe) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

[ ]  3. Clean the battery.

 [ ]  4. Clean the battery cables and cable ends.

 [ ]  5. Remove and install the battery.

 [ ]  6. Perform any required battery reset procedures.

