[ ]  1. Check service information for the specified replacement procedure for the vehicle being serviced. \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Evaluation (Enter number from 4, 3, 2, 1) :\_\_\_\_\_\_\_\_\_

Meets ASE Task: A5 – F-6 – P-1

Time on Task:\_\_\_\_\_\_\_\_\_\_\_\_\_

Make/Model/Year:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

VIN:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_

Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Sealed Wheel Bearing Replacement**

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

[ ]  2. Safely hoist the vehicle.

[ ]  3. Remove the front wheel.

 [ ]  4. Remove the drive axle shaft hub nut.

 [ ]  5. Remove the front disc brake caliper.

 [ ]  6. Remove the rotor, the hub, and splash shield retaining bolts.

 [ ]  7. Mark the location of the hub and make certain the hub is loose on the steering knuckle.

 [ ]  8. Install the hub puller and remove the bearing and hub assembly.

 [ ]  9. Clean and lubricate hub bearing surface.

 [ ]  10. Install the hub and bearing assembly

 [ ]  11. Torque the drive axle shaft nut to specification.

 Specification = \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ (usually about 200 lb.-ft.)

 [ ]  12. Reinstall the rotor, caliper, and wheel.

