[ ]  1. Check service information for the recommended procedures and specifications for checking vacuum supply to power booster.

Evaluation (Enter number from 4, 3, 2, 1) :\_\_\_\_\_\_\_\_\_

Meets ASE Task: A5 – E-3 – P-2

Time on Task:\_\_\_\_\_\_\_\_\_\_\_\_\_

Make/Model/Year:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

VIN:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_

Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Vacuum Supply/Manifold or Auxiliary Pump**

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

[ ]  2. Is the vehicle equipped with an auxiliary vacuum pump? [ ] \_\_\_\_ Yes [ ] \_\_\_\_ No

[ ]  3. Most vehicle manufacturers specify that a vacuum “T” be installed in the vacuum line between the intake manifold and/or auxiliary pump and the vacuum power brake booster assembly. Most manufacturers specify a minimum of 15 in. Hg. of vacuum be measured.

 Actual vacuum measured at the power brake booster = \_\_\_\_\_\_\_\_\_\_

 [ ] \_\_\_\_ OK [ ] \_\_\_\_ NOT OK

