Tire Replacement

Meets ASE Task: (A4-F-6) P-1 Dismount and remount tire on wheel; balance.

**Name \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date \_\_\_\_\_\_\_\_\_\_\_ Time on Task \_\_\_\_\_\_\_\_\_\_**

**Make/Model/Year \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ VIN \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Evaluation: 4 3 2 1**

\_\_\_\_\_ 1. Check the instructions for the proper use of the tire changer. Describe the


recommended procedure.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_ 2. Check all steps that were performed.

\_\_\_\_ Removed the valve core (TPMS equipped tire/wheel assembly; check

 service information for the exact procedure to follow.)

\_\_\_\_ Demount the tire from the wheel. Instructor OK \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 \_\_\_\_ Clean bead seat.

\_\_\_\_ Lubricate the tire bead.

\_\_\_\_ Mount the tire and inflate to

specified inflation pressure.

\_\_\_\_\_ 3. Balance tire/wheel assembly.

Instructor OK \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_