**Meets ASE Task:** (A5-B-5) P-1 Select, handle, store, and fill brake fluids to proper level; use proper fluid type per manufacturer specification. (A5-B-13) P-1 Test brake fluid for contamination.

Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_

Time on Task:\_\_\_\_\_\_\_\_\_\_\_\_\_

Make/Model/Year:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

VIN:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Evaluation (Enter number from 4, 3, 2, 1) :\_\_\_\_\_\_\_\_\_

**Brake Fluid**

Page 300

[ ]  **1.** Check service information for the specified brake fluid and when to check for the

 proper level.

 A. Specified brake fluid = \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 B. Specified brake fluid level \_\_\_\_\_\_\_\_\_ (describe the location) \_\_\_\_\_\_\_\_\_\_\_\_\_

****

[ ]  **2.** Check service information for the recommended procedure to follow to determine if

 the brake fluid is contaminated. Describe the specified procedure:

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

[ ]  **3.** Check all that apply according to service information.

 [ ]  Perform a visual inspection.

 [ ]  Place the sample in Styrofoam cup and check for eating away of the cup at

 the top of the fluid level line.

 [ ]  Use a test strip.

 [ ]  Use a brake fluid boiling temperature tester

 [ ]  Other (describe) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_