Evaluation (Enter number from 4, 3, 2, 1) :\_\_\_\_\_\_\_\_\_

**Meets ASE Task:** (A0-C-4) Perform a vehicle multi-point inspection and complete a vehicle inspection report.

**Safety Check**

Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_

Time on Task:\_\_\_\_\_\_\_\_\_\_\_\_\_

Make/Model/Year:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

VIN:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Page 32

 **1.** Check the headlights (high and low).

**2.** Check the taillights.

**3.** Check the side marker lights.

**4.** Check the license plate light.

**5.** Check the brake lights.

**6**. Check the turn signals.

**7.** Check the back-up lights with the ignition switch "on" (engine "off") and the gear

selector in reverse.

**8.** Check the windshield wipers (all speeds) and wiper blades.

**9.** Check the heater-defroster fan (all speeds).

**10.** Check the condition of the tires (must have at least 2/32" of tread) and the tire

pressure. Do not forget to check the spare tire!

**11.** Check for looseness in the steering wheel (less than 2" of play).

**12.** Check the 4-way emergency flashers.

**13.** Check the horn.

**14.** Listen for exhaust system leaks.

**15.** Check the parking brake (maximum 8-10 "clicks" and should "hold" in drive).