Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_

Time on Task:\_\_\_\_\_\_\_\_\_\_\_\_\_

Make/Model/Year:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

VIN:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Evaluation (Enter number from 4, 3, 2, 1) :\_\_\_\_\_\_\_\_\_

**Meets ASE Task: :** (A4-D-1) P-1 Inspect, remove, and/or replace shock absorbers; inspect mounts and bushings.

**Front Shock Absorber Replacement**

Page 350

**[ ]  1.** Verify that the front shock absorber requires replacement. Check all that apply:

 **[ ]** bent or damaged shock or mounting hardware

 **[ ]** shock absorber is leaking hydraulic fluid

 **[ ]** excessively worn - causing tire wear or riding comfort problems

 **[ ]** other (specify) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**[ ]  2.** Compare the replacement shocks to the original shocks to be sure that they are correct.

 **OK [ ]  NOT OK [ ]**

**NOTE:** All shock absorbers should be replaced in pairs only. Do not replace just one shock absorber.

**[ ]  3.** Check the service information for the specified replacement procedure. \_\_\_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**HINT:** Many shocks on rear-wheel-drive vehicles can be broken off using a

deep-well socket and a long extension. By rocking the extension back and forth, the top of the shock will usually break off saving the time and effort it takes to remove a nut that is often rusted in place after many years of service.

**[ ]  4.** Safely hoist the vehicle.

**[ ]  5.** Remove the lower shock absorber retaining bolts (nuts) as per the service information

 instructions..

**CAUTION:** Be ready to catch the shock absorber because it will likely fall after removing the last retaining bolt (nut).

**[ ]  6.** Show the instructor the removed shock absorber**. Instructor’s OK \_\_\_\_\_\_\_\_\_\_\_\_\_**

**[ ]  7.** Extend the rod on the replacement shock and install the lower retaining bolts (nuts).

**[ ]  8.** Lower the vehicle and install the upper retaining fastener.

**[ ]  9.** Bounce the vehicle to check that the replacement shock does not interfere with any

 part of the suspension or frame.

**[ ]  10.** Test drive the vehicle before returning it to the customer.