Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_

Time on Task:\_\_\_\_\_\_\_\_\_\_\_\_\_

Make/Model/Year:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

VIN:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Evaluation (Enter number from 4, 3, 2, 1) :\_\_\_\_\_\_\_\_\_

**Meets ASE Task: :** (A3-F-4) P-3 Check for leaks at drive assembly and transfer case seals; check vents; check fluid level; use proper fluid type per manufacturer specification.

**Four-Wheel Drive Fluid**

Page 415

**[ ]  1.** Check the service manual for correct fluid and for the location for inspecting the fluid.

  **Recommended fluid = \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Inspection location = \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**



**[ ]  2.** Hoist the vehicle safely.

**[ ]  3.** Inspect the fluid level and replace as

 required or recommended.

**[ ]** level okay

**[ ]** level low - added fluid

**[ ]** drained and replaced the fluid

**[ ]  4.** Check the engine and transmission/transfer

 case mounts.

**[ ]** all mounts are dry and okay

**[ ]** one or more of the mounts is oil soaked

**[ ]** one or more of the mounts is collapsed or defective

**[ ]** other (describe) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**NOTE:** A defective engine or transmission/transfer case mount can cause abnormal vibrations and noise.