Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_

Time on Task:\_\_\_\_\_\_\_\_\_\_\_\_\_

Make/Model/Year:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

VIN:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Evaluation (Enter number from 4, 3, 2, 1) :\_\_\_\_\_\_\_\_\_

**Meets ASE Task: :** (A3-F-4) P-3 Check for leaks at drive assembly and transfer case seals; check vents; check fluid level; use proper fluid type per manufacturer specification.


**Four-Wheel Drive Fluid**

Page 415

**1.** Check the service manual for correct fluid and for the location for inspecting the fluid.

**Recommended fluid = \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Inspection location = \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**



**2.** Hoist the vehicle safely.

**3.** Inspect the fluid level and replace as

required or recommended.

level okay

level low - added fluid

drained and replaced the fluid

**4.** Check the engine and transmission/transfer

case mounts.

all mounts are dry and okay

one or more of the mounts is oil soaked

one or more of the mounts is collapsed or defective

other (describe) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**NOTE:** A defective engine or transmission/transfer case mount can cause abnormal vibrations and noise.