Evaluation (Enter number from 4, 3, 2, 1) :\_\_\_\_\_\_\_\_\_

**Meets ASE Task:** (A1-A-8) P-2 Identify service precautions related to service of an internal combustion engine of a hybrid vehicle.

**Hybrid Electric Vehicle Safety Precautions**

Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_

Time on Task:\_\_\_\_\_\_\_\_\_\_\_\_\_

Make/Model/Year:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

VIN:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Page 42

**[ ]  1.** Check service information for the specified procedures to follow when servicing the

 engine of a hybrid electric vehicle. Describe the specified precautions. \_\_\_\_\_\_\_\_\_\_

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**[ ]  2.** Does the vehicle need to have the high-voltage disconnect removed before changing the engine oil?

 **[ ]** Yes **[ ]** No

**[ ]  3.** Check the location of the following:

 **[ ]** High-voltage orange cables

 **[ ]** High-voltage yellow or blue conduit wiring

 **[ ]** High-voltage A/C compressor

 **[ ]** High-voltage disconnect

**[ ]** Other (describe) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**[ ]  4.** Describe the location of the following:

 High-voltage \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Orange cables \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_