Evaluation (Enter number from 4, 3, 2, 1) :\_\_\_\_\_\_\_\_\_

**Meets ASE Task:** (A1-D-2) P-1 Perform engine oil and filter change; use proper fluid type per manufacturer specification; reset maintenance reminder as required.

**Engine Oil Change**

Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_

Time on Task:\_\_\_\_\_\_\_\_\_\_\_\_\_

Make/Model/Year:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

VIN:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Page 58

**1.** Check the owner's manual, service manual, or technical literature to determine the

correct viscosity rating and quantity of oil needed.

1. Recommended viscosity: SAE \_\_\_\_\_\_\_ or SAE \_\_\_\_\_\_\_\_
2. Number of quarts (liters): with the filter \_\_\_\_\_\_ without the filter \_\_\_\_\_\_
3. American Petroleum Institute rating (if specified) \_\_\_\_\_\_\_\_\_\_\_

**2.** Filter brand and number: Brand \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Number \_\_\_\_\_\_\_\_\_\_\_\_\_

**3.** Hoist the vehicle safely. Position the oil drain unit under the drain plug and raise to a

height about 1 foot under the drain plug.

**4.** Select the proper size wrench and remove the drain plug and allow the oil to drain into

the drain pan.

**5.** After all the oil has been drained, install a new sealing washer (if needed) and install

the drain plug.

**6.** Move the oil drain unit under the filter and remove the old oil filter.

**7.** Use a shop cloth and clean the oil filter gasket contact area on the engine block.

**8.** Apply a thin coating of engine oil to the rubber gasket on the new oil filter.

**9.** Install the new oil filter and hand tighten about 3/4 turn after the gasket contacts the

engine block.

**10.** Lower the vehicle. Install the recommended quantity of engine oil using a funnel to

prevent spilling oil. Replace the oil filler cap.

**11.** Start the engine and allow it to idle. The "oil" light should go out within 15 seconds.

**12.** Look under the vehicle and check for leaks at the drain plug and the oil filter.

**13.** Check the level of the oil again and add as needed. **Caution:** Do not overfill!